{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["4 设备采购和安装采购清单"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"4 设备采购和安装采购清单","index":0,"n_rows":65,"n_cols":10,"rows_kept":65,"merged":[[0,2,0,9],[1,2,1,7],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,9,3,9],[63,2,63,3],[63,7,64,9],[64,2,65,3]]}
[null,null,"设备采购分类分项工程量清单计价表",null,"","","","","",""]
[null,null,"工程名称：洪泽湖周边滞洪区近期建设工程（泗洪县）施工16标",null,"","","","","",""]
[null,null,"序号","项目名称","项目特征描述","计量单位","工程数量","单价（元）","合价（元）","备注"]
[{"$nulls":4},"","","","小计","合计",""]
[null,null,"1","水利安装工程","","","",""]
[null,null,"1.10","金属结构-红旗应山1号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.10.1.1.1","红旗应山1号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.10.1.2.1","红旗应山1号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、不锈钢罩壳等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.11","金属结构-红旗应山2号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.11.1.1.1","红旗应山2号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.11.1.2.1","红旗应山2号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、不锈钢罩壳等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.12","金属结构-金圩村1号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.12.1.1.1","金圩村1号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1]
[null,null,"1.12.1.1.2","金圩村1号涵闸检修闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.12.1.2.1","金圩村1号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.12.1.2.2","金圩村1号涵闸检修闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.13","金属结构-孙庄村2号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.13.1.1.1","孙庄村2号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.13.1.1.2","孙庄村2号涵闸检修闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.13.1.2.1","孙庄村2号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.13.1.2.2","孙庄村2号涵闸检修闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.14","金属结构-孙庄村1号涵闸","2.0m（宽）×2.0m（高）×2（孔）涵闸","","",null,null,""]
[null,null,"1.14.1.1.1","孙庄村1号涵闸工作闸门","ZMQJ-2000X2000-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",2,null,null,""]
[null,null,"1.14.1.1.2","孙庄村1号涵闸检修闸门","ZMQJ-2000X2000-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",2,null,null,""]
[null,null,"1.14.1.2.1","孙庄村1号涵闸工作闸门启闭机","QLW-80kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",2,null,null,"含配套电控箱"]
[null,null,"1.14.1.2.2","孙庄村1号涵闸检修闸门启闭机","QLW-80kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",2,null,null,"含配套电控箱"]
[null,null,"1.15","金属结构-勒东村1号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.15.1.1.1","勒东村1号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.15.1.1.2","勒东村1号涵闸检修闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.15.1.2.1","勒东村1号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.15.1.2.2","勒东村1号涵闸检修闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.16","金属结构-马坟站涵洞","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.16.1.1.1","马坟站涵洞工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1]
[null,null,"1.16.1.1.2","马坟站涵洞检修闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.16.1.2.1","马坟站涵洞工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.16.1.2.2","马坟站涵洞检修闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.17","金属结构-勒东村2号涵闸","1.5m（宽）×1.5m（高）×1（孔）涵闸","","",null,null,""]
[null,null,"1.17.1.1.1","勒东村2号涵闸工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.17.1.1.2","勒东村2号涵闸检修闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.17.1.1.3","勒东村2号涵闸出水口工作闸门","自撑式铸铁闸门ZMQJ-1300X1300-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.17.1.2.1","勒东村2号涵闸工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.17.1.2.2","勒东村2号涵闸检修闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.17.1.2.3","勒东村2号涵闸出水口工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.18","金属结构设备-东咀1号站","55kw×1台套泵站","","",null,null,""]
[null,null,"1.18.1","金属结构设备采购及安装工程","","","",null,null,""]
[null,null,"1.18.1.1.1","东咀1号站上道工作闸门","ZMQJ-2300X1300-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.18.1.1.2","东咀1号站下道工作闸门","ZMQJ-2300X1800-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",2,null,null,""]
[null,null,"1.18.1.1.3","东咀1号站灌溉孔工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.18.1.1.4","东咀1号站泵站拦污栅","2.3×2.0m钢格栅(Q235焊接件，含滑块、喷锌防腐等，每扇约重1.1t)，含吊装等","扇",1,null,null,""]
[null,null,"1.18.1.1.5","东咀1号站洞首工作闸门","ZMQJ-1500X1500-5m；材质：HT250；止水：铜条止水；含轨道门框及预埋件，按DB32/T1712-2011设计制造","扇",1,null,null,""]
[null,null,"1.18.1.1.6","东咀1号站洞首拦污栅","1.5×2.0m钢格栅(Q235焊接件，含滑块、喷锌防腐等，每扇约重0.8t)，含吊装等","扇",1,null,null,""]
[null,null,"1.18.1.2","门槽埋件制造及安装","","","",null,null,""]
[null,null,"1.18.1.2.1","东咀1号站泵站检修闸门埋件","闸孔净宽2.3m，闸墩高度6.4m( Q235焊接件，二期砼预埋安装，含主轨、反轨、喷锌防腐等)","t",0.63,null,null,""]
[null,null,"1.18.1.2.2","东咀1号站洞首检修闸门埋件","闸孔净宽1.5m，闸墩高度7.3m( Q235焊接件，二期砼预埋安装，含主轨、反轨、喷锌防腐等)","t",0.72,null,null,""]
[null,null,"1.18.1.2.3","东咀1号站泵站拦污栅埋件","闸孔净宽2.3m，闸墩高度2.0m( Q235焊接件，二期砼预埋安装，含主轨、反轨、喷锌防腐等)","t",0.22,null,null,""]
[null,null,"1.18.1.2.4","东咀1号站洞首拦污栅埋件","闸孔净宽1.5m，闸墩高度2.0m( Q235焊接件，二期砼预埋安装，含主轨、反轨、喷锌防腐等)","t",0.22,null,null,""]
[null,null,"1.18.1.3","其它设备采购及安装","","","",null,null,""]
[null,null,"1.18.1.3.1","东咀1号站上道工作闸门启闭机","QLW-80kN手电两用螺杆式启闭机，含启闭机架、预埋件、不锈钢防雨罩壳等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.18.1.3.2","东咀1号站下道工作闸门启闭机","QLW-80kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架、不锈钢防雨罩壳等","台套",2,null,null,"含配套电控箱"]
[null,null,"1.18.1.3.3","东咀1号站灌溉孔工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、不锈钢防雨罩壳等","台套",1,null,null,"含配套电控箱"]
[null,null,"1.18.1.3.4","东咀1号站洞首工作闸门启闭机","QLW-50kN手电两用螺杆式启闭机，含启闭机架、预埋件、轴导架等","台套",1,null,null,"含配套电控箱"]
[{"$nulls":3},"合计","","","",null,null,""]
[]
[null,null,"投标人：        （盖章）",{"$nulls":4},"日期：","",""]
[null,null,"法定代表人或委托代理人：             （签字或盖章）",{"$nulls":5},"",""]